|  |  |  |
| --- | --- | --- |
| Cost | Name | Use |
| 10.93 | Adafruit Pro trinket 5v board |  |
| 9.13 | Maxim Max 7219 CNG |  |
| .99 | TP223 Capacitive Touch | Uses capacitive touch as a sensor that works with the code |
| 18.74 | Colored Hook-up Wire |  |
| 2.68 x 3 | 3 bars |  |
| 8.49 | 5V DC Power Adapter (wall wort) |  |
| 6.33 | Panel mount 5V DC Power Jack | https://www.amazon.com/BQLZR-Supply-Adapter-Socket-Single/dp/B00EQ1UWX4/ref=sr\_1\_cc\_1?s=aps&ie=UTF8&qid=1484691217&sr=1-1-catcorr&keywords=BQLZR+5.5mm+X+2.1+DC+Power |
| 6.99 | XLR female conector | Hand held piece |
| 2.00 | XLR male panel mount | Box side connection for hand held controller |
| 10.95 | XLR Patch cable |  |
| 23.25 | 45 watt soldering iron |  |
| 9.21 | Roll of solder |  |
| 7.98 | Flux pins |  |
| $11 | ¼” audio cable | Strong cables that work for the capacitance. |